# 231901043

# RITHUPRIYA.S

**EXP NO:1A**

**DATE:27.7.24**

**BASIC NETWORKING COMMANDS IN WINDOWS OPERATING**

**SYSTEM**

**Aim:**

To study the basic commands operating system in window operating system.


**1. IPCONFIG**

The IPCONFIG network command provides a comprehensive view of information regarding the [IP address co](https://www.simplilearn.com/tutorials/cyber-security-tutorial/what-is-an-ip-address)nfiguration of the device we are currently working on.

The IPConfig command also provides us with some variation in the primary command that targets specific system settings or data, which are:

* IPConfig/all - Provides primary output with additional information about network adapters.
* IPConfig/renew - Used to renew the system’s IP address.
* IPConfig/release - Removes the system’s current IP address.

SYNTAX- ipconfig EXAMPLE : ipconfig OUTPUT:



1. **NSLOOKUP**

The NSLOOKUP command is used to troubleshoot network connectivity issues in the system. Using the nslookup command, we can access the information related to our system’s DNS server, i.e., domain name and IP address.

Syntax– nslookup

Example : nslookup [www.google.com](http://www.google.com/)


OUTPUT:



1. **HOSTNAME**

The HOSTNAME command displays the hostname of the system. The hostname command is much easier to use than going into the system settings to search for it.

SYNTAX- hostname EXAMPLE : hostname OUTPUT:



1. **PING**


The Ping command is one of the most widely used commands in the prompt tool, as it allows the user to check the connectivity of our system to another host.

This command sends four experimental packets to the destination host to check whether it receives them successfully, if so, then, we can communicate with the destination host. But in case the packets have not been received, that means, no communication can be established with the destination host.

SYNTAX- ping www.destination\_host\_name.com

EXAMPLE : ping [www.facebook.com](http://www.facebook.com/)

OUTPUT:




1. **TRACERT**

The TRACERT command is used to trace the route during the transmission of the data packet over to the destination host and also provides us with the “hop” count during transmission. Using the number of hops and the hop IP address, we can troubleshoot network issues and identify the point of the problem during the transmission of the data packet.

SYNTAX- tracert IP-address OR tracert www.destination\_host\_name.com

EXAMPLE : tracert [www.facebook.com](http://www.facebook.com/)

OUTPUT:




1. **NETSTAT**

The Netstat command as the name suggests displays an overview of all the network connections in the device. The table shows detail about the connection protocol, address, and the current state of the network.

SYNTAX- netstat EXAMPLE

: netstat

OUTPUT:




1. **ARP(Address Resolution Protocol)**

The ARP command is used to access the mapping structure of IP addresses to the MAC address. This provides us with a better understanding of the transmission of packets in the network channel.

SYNTAX- arp

EXAMPLE : arp -a

OUTPUT:





1. **SYSTEMINFO**

Using the SYSTEMINFO command, we can access the system’s hardware and software details, such as processor data, booting data, Windows version, etc.

SYNTAX– systeminfo

EXAMPLE : systeminfo

OUTPUT;




1. **ROUTE**

Provides the data of routing data packets in the system over the communication channel.

SYNTAX – route print EXAMPLE

: route print

OUTPUT:



# RESULT

Hence, the study of basic networking commands in window operating system is studied.